
**Timing**


**Exercise 1 –** You would like to find the propagation delay and contamination delay of the circuit shown in figure Below. According to his data book, each gate has a propagation delay of 100 picoseconds (ps) and a contamination delay of 60 ps.




Solution:

Start finding the critical path and the shortest path through the circuit.


In the critical path tpd is three times the propagation delay of a single gate, or 300 ps.





The shortest path are only two gates in the shortest path, so tcd is 120 ps.



**Exercise 2 –** Compare the worst-case timing of the three four-input multiplexer designs shown in the two figure below. The table lists the propagation delays for the components. What is the critical path for each design? Given your timing analysis, why might you choose one design over the other?




Solution:

One of the critical paths for each of the three design options is highlighted in blue.

tpd\_sy indicates the propagation delay from input S to output Y;

tpd\_dy indicates the propagation delay from input D to output Y;

tpd for the circuit is the worst of the two: max(tpd\_sy, tpd\_dy).



For both the two-level logic and tristate implementations in figures,

the critical path is from one of the control signals S to the output Y: tpd = tpd\_sy.

These circuits are control critical, because the critical path is from the control signals to the output.


Any additional delay in the control signals will add directly to the worst-case delay.

The delay from D to Y in Figure (b) is only 50 ps, compared with the delay from S to Y of 125 ps.

The best choice depends not only on the critical path through the circuit and the

input arrival times but also on the power, cost, and availability of parts.

**Exercise 3 –** Determine the propagation delay and contamination delay of the circuit in the following figure. Use the gate delays given in Table.

****

**Immagine che contiene tavolo

Descrizione generata automaticamente**

Solution:

Start finding the critical path and the shortest path through the circuit.


In the critical path tpd is the sum of the propagation delays, so tpd is 150 ps.

The shortest path are only two gates in the shortest path, so tcd is 65 ps.


**Exercise 4 –**


Immagine che contiene piazza


Descrizione generata automaticamente



**Exercise 5 –**







**Exercise 6 –**A circuit has gets with propagation and contamination delays of 0.61 ns and 0.30 ns, respectively. It also contains flip-flops with propagation and contamination delays of 0.72 and 0.50 ns, and setup and hold times of 0.53 ns and 0 ns, respectively.

(a) If you are building a system that needs to run at 40 MHz, how many consecutive gates can you use between two flip-flops? Assume that there is no clock skew and no delay through wires between gates.

(b) Suppose that all paths between flip-flops pass through at least one gate. How much clock skew can the circuit have without violating the hold time?

Solution:  
(a) *Tc* = 1 / 40 MHz = 25 ns

*Tc* **≥** *tpcq + Nt*CLB *+ t*setup

25 ns **≥** [0.72 + *N*(0.61) + 0.53] ps

Thus, N < 38.9

**N = 38**

(b)

*t*skew < (*tccq + tcd\_*CLB*)* - *t*hold

< [(0.5 *+* 0.3*)* - 0] ns

**< 0.8 ns = 800 ps**

**Exercise 7 –** You would like to build a synchronizer that can receive asynchronous inputs with an MTBF of 50 years. Your system is running at 1 GHz, and you use sampling flip-flops with τ = 100 ps, T0 = 110 ps, and tsetup = 70 ps. The synchronizer receives a new asynchronous input on average 0.5 times per second (i.e., once every 2 seconds). What is the required probability of failure to satisfy this MTBF? How many clock cycles would you have to wait before reading the sampled input signal to give that probability of error?

Solution:

P(failure)/sec = 1/MTBF = 1/(50 years \* 3.15 x 107 sec/year) = **6.34 x10-10**

P(failure)/sec waiting for one clock cycle: N\*(T0/Tc)\*e-(Tc-tsetup)/Tau

= 0.5 \* (110/1000) \* e-(1000-70)/100 = 5.0 x 10-6

P(failure)/sec waiting for two clock cycles: N\*(T0/Tc)\*[e-(Tc-tsetup)/Tau]2

= 0.5 \* (110/1000) \* [e-(1000-70)/100]2 = 4.6 x 10-10

This is just less than the required probability of failure (6.34 x 10-10).

Thus, **2 cycles** of waiting is just adequate to meet the MTBF.